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g four-figure grid references on a m:

Ordnance Survey (OS)
maps have faint blue

-3 lines over the top of
\7 them. These are called
N el gridlines. We can use
, WHITLEY BAY

A b these to help us locate
places on a map.
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Northings are horizontal lines

ﬂ/ on a map that run from left to
right. The numbers on the
lines increase as you move
north.

Together, eastings and northings create a grid that helps us pinpoint
specific locations on a map. @
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references on a m:
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Eastings are vertical lines on a

JHTLEY BAY

map that run from the bottom
~ to the top. The numbers on the
lines increase as you move

east.
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To find the number of

the grid square, we

ook at the bottom left

corner of the square

we want to locate.

square we want
to find the
number for

the bottom left
corner
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To find the four-figure grid
reference we first go east ‘along
the corridor’ and look for the
number on the line that forms the
left-hand side of the box.
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We then go north ‘up the
stairs” and find the number
at the bottom of the square
we want.

We put these numbers
together to create a four-
figure grid reference: 3474.





